1. Thermal performance of double-layer porous copper strips mounted as hollow cylinders

Alrubaiy, A.A., Al-Bakri, B.A.R., Aljuhashy, R.M. Periodicals of Engineering and Natural Sciences, 2021, 9(2), pp. 784–798

1. Effect of Operating Conditions on The Performance of Shell and Tube Service Condenser. Alrubaiy, A.A., Al-Bakri, B.A.R., Aljuhashy, R.M. Journal of Mechanical Engineering Research & Developments,2021, Vol. 44, No. 8, pp. 175-187
2. CO2 laser spot welding of thin sheets AISI 321 austenitic stainless steel

Shehab, A.A., Nawi, S.A., Al-Rubaiy, A.A.A.G., ...Alali, M.S., Ali, S.D. Archives of Materials Science and Engineeringthis link is disabled, 2020, 106(2), pp. 68–77

1. Experimental And Computational Investigation Of Flame Holders In Combustion Chambers At Different Thermal Loads Alhumairi, M.K.A., Yahya, S.G., Azzawi, I.D.J., Al-Rubaiy, A.A. Journal of Thermal Engineering, 2020, 6(6), pp. 369–378
2. Characteristics of acoustic drivers for efficient coupling to thermoacoustic machines. Yahya, S.Gh., Azzawi, I.D.J., Abbas, M.K., Al-Rubaiy, A.A.A.G. Lecture Notes in Engineering and Computer Science, 2019, 2239, pp. 469–474